**VAN BUREN STREET – SOUTH SIDE (EVEN)**

**204 Van Buren Street c.1959**

**Two-story garrison colonial frame house on large lot with side gable roof and broad central chimney** Front façade is symmetrical three-bay composition: center front door with sidelights, with 28-lite picture sash to either side. Three double-hung sash at second floor front. Windows are primarily 8/8 double-hung wood sash in varying sizes with decorative louvered shutters. Two-and-one-half bay side-gable attached garage recessed to right has overhead rolling door. Concrete block foundation, wood clapboard siding and asphalt shingle roofing. Concrete driveway.

**208 Van Buren Street c. 1908**

**Two-story frame house with broad steeply pitched side gambrel roof**

Full-width front porch with low-pitched shed roof, modern posts, balustrade, and floor; porch shelters front door to left and window bay to right. Center second-floor dormer beneath upper pitch of gambrel contains two sash. Windows are generally 1/1 double-hung replacement sash. Rubble-stone foundation, vinyl siding at first floor with wood shingle siding above in gambrel, and asphalt shingle roofing. Contributing single-bay frame garage with wood clapboard siding; concrete driveway.

**210 Van Buren Street c.1919**

**One-and-one-half story house with low jerkinhead side-gable roof**

Primary façade is symmetrical three-bay composition with paired 12-lite entry doors at center, 12-lite French doors and transom to either side. Center entrance has broad surround, segmented arch pediment above, brick stoop with wrought iron railings, and small 3-lite side casements. Three shed-roof dormers containing 8-lite casement sash align with doors below; center dormer is the broadest of the three. Sun room wing to right (west) has low-slope roof, broad eaves and paneled walls with large multi-lite steel sash. Windows are generally casement sash with thick sills and jack-arch lintels at first floor expressed in stucco wall finish. Stucco walls with brick soldier course at grade and asphalt shingle roofing.

Contributing two-bay jerkinhead gable roof garage with stucco cladding, wood clapboard at gable, and modern overhead door. Cast concrete driveway with integrated curb, shared with 212 Van Buren Street, appears to be period.

**212 Van Buren Street c.1920**

**Two-story frame house with side gable roof and two stucco clad chimneys**

Primary façade is symmetrical three-bay composition: center entrance has sidelights, pilasters, arched hood on corbels, and decorative reeded elliptical spandrel above. To either side of entrance is a pair of 8-lite French doors with paneled wood shutters. Second-floor windows are primarily 6/1 double-hung wood sash with cut-out and louvered wood shutters. Nearly full-width side porch at left has shed roof, dentilated cornice, paired square classical columns, modern enclosure, and modern solarium extension. Stucco walls and asphalt shingle roofing.

Contributing two-bay hip-roof frame garage has stucco walls, modern overhead door, and asphalt shingle roofing.

**VAN BUREN STREET – NORTH SIDE (ODD)**

**201 Van Buren Street c.1909**

**Two-story frame house with gable roof**

**Front façade is nearly symmetrical**

Full-width front porch has square posts, closely spaced square wood balusters, and low-pitched roof. Porch shelters slightly off-center projecting entry door with paired 1/1 double-hung windows to either side. Second-floor front has paired sash aligned with sash below. Flat-top Palladian window in gable. Windows are primarily 1/1 double-hung replacement sash. Left (west) side has hip-roof window bay at first floor. Stone foundation, vinyl siding, and asphalt shingle roofing. Asphalt driveway.

**203 Van Buren Street c.1908**

**Two-story frame house with hip roof**

Full-width front porch with low-slope roof, square columns, pediment over entry steps, modern enclosure of left two-thirds with 8/8 double-hung sash, and entry door with sidelights beneath. Second-floor front has door at left and pair of sash to right. Front eyebrow dormer infilled with siding. Windows are primarily 1/1 double-hung replacement sash. West side has two-story window bay. Rough ashlar block foundation, aluminum siding, and asphalt shingle roofing. Terraced yard; modern lumber retaining wall. Set of four concrete steps with metal pipe handrail.

Contributing one-story frame garage with gable roof; concrete driveway with concrete curbs.

**205 Van Buren Street c.1920**

**Two-story frame house with hip roof, half-width front cross gable, side gable-roofed dormers, and brick chimney**

First floor front is three-bay porch, flush with façade rather than projecting. Porch is divided by paired square fluted columns on stone piers. Left two bays have period enclosure with three 8-lite sash on paneled wood balustrade; right bay has projected portico on round fluted columns over stone entry stoop, behind which front door is recessed and has leaded glass sidelights. Two paired second-floor front windows. Semi-lunette sash in front gable. Windows are predominantly single or paired 1/1 double-hung wood sash. Left façade has first floor window bay, and right façade has one-story cascading gable roof addition. Ashlar stone foundation, wood clapboard siding, and asphalt shingle roofing.

Contributing two-bay gable roof garage with raised cross gable, wood clapboard siding, modern overhead doors and asphalt shingle roofing; concrete driveway with concrete curb.

**207 Van Buren Street c.1910**

**Two-story frame house with side-gable roof and half-width front cross gable, projected bargeboard on triangular brackets, and exposed rafter tails**

Full width front porch with low-pitched hip roof, left two-thirds width enclosure in clapboard siding and banks of 12-lite casement sash, recessed entry with modern post railing and steps. Porch sits on modern concrete block foundation incorporating a one-bay garage. Second-floor front windows are paired 6/6 double hung sash. 18-lite fixed sash in front cross-gable and in front gable-roofed dormer. Left (west) side has first-floor window bay. Windows are primarily multi-lite modern wood doublehung sash of varying sizes. Stone foundation (except beneath porch), wood clapboard siding at first floor with wood shingle siding above, and asphalt shingle roofing. Current owner has recently undertaken a large scale rehabilitation of the exterior removing vinyl siding and inappropriate replacement sash, and reconstructing millwork details.

Contributing two-bay gable roof garage with wood clapboard siding, and asphalt shingle roofing. Asphalt driveway to detached garage; concrete driveway to integral garage.

**209 Van Buren Street c.1927**

**Two-story frame house with L-shaped footprint**

**Cross-hip roof slopes down to first floor at left; large brick chimney with corbelled crown**

Front façade has coordinated asymmetrical arrangement of paired sash. No entrances on front of house; entrances are on east side beneath cross gable and at side porch located on the west side. Windows are primarily paired steel casement sash with leaded-glass panes (rectangular paned at first floor, diamond paned at second floor). First floor is clad in brick; second floor stucco with faux wood timbering and intermittent use of wood siding.

Contributing three and one-half bay garage with tall hip roof, arched pedestrian door with decorative strap hinges, period multi-lite overhead doors, and stucco cladding is connected to house with breezeway. Asphalt driveway.

**213 Van Buren Street c.1915**

**Two-story frame house with American Foursquare form**

Nearly full width front porch has tapered square columns on rock-faced concrete block piers, wood balustrade, pointed-arch spandrels, and shaped corbels. Porch shelters entry door to left, Chicago-style window to right. Two second-floor front windows. Front and side hip-roofed dormers contain triple windows. Right (east) side has first-floor bay window. Windows are a mix of 1/1 double-hung and fixed replacement sash. Rock-faced concrete block foundation, vinyl siding, and asphalt shingle roofing. Vinyl siding recently installed over original wood clapboard and shingle siding. Terraced yard; low informal stone retaining wall; set of three concrete steps.