**CHESTNUT STREET – SOUTH SIDE (EVEN)**

**12 Chestnut Street c. 1900**

**Two-story frame house with hipped roof and slightly projecting front cross-gable; modest Queen Anne/Free Classic character.**

 Full-width hip-roofed front porch on concrete block foundation has square wood posts and deck-style wood railing. Porch shelters center entrance in projecting vestibule, with one 1/1 window to either side. Cutaway corner with decorative scrolled brackets and corner drop at front left (northeast) corner. Front

hip-roofed dormer, side gable-roofed dormers, containing decorative wood windows. Asbestos shingle siding; asphalt shingle roof. Below-grade concrete block addition, previously used as a garage, extends to the west. Terraced yard; set of four brick and concrete steps with metal pipe handrail.

**14 Chestnut Street c. 1900**

**Two-story frame house with closed-gable roof; modest Queen Anne/Free Classic character.**

Full-width front porch with square posts, replacement railing, dentils at cornice, and pediment over center stairs. Porch shelters off-center front door and two 1/1 front windows. Two off-center second-floor front windows, each 6/6 doublehung sash; irregular window placement suggests one window may be missing. Chicago-style window in gable. Front gable and side cross-gables contain wood fishscale shingles. Asbestos shingle siding; asphalt shingle roof. Terraced yard; brick retaining wall; set of five concrete steps with metal rail.

**18 Chestnut Street c. 1900**

**Two-story frame house with Queen Anne/Free Classic character.**

Hipped roof with projecting cross gables at front and west sides. Full-width front porch with square posts and wood balustrade has hipped roof and dentils at cornice. Second-floor front windows are casements with unusual decorative pattern. Recessed porch set in arched opening at attic level of west cross gable. Attached one-story garage at southwest corner. Wood clapboard siding; asphalt shingle roof. Terraced yard; set of five concrete steps. Asphalt driveway.

**20 Chestnut Street c. 1902-11**

**One-story frame bungalow; broad side-gabled roof with deep overhanging eaves.**

Full-width porch is sheltered beneath main roof; porch has solid sided rail and wide square columns. Porch shelters front door with sidelights, with 1/1 double-hung window to either side. Center front shed-roofed dormer contains two 1/1 double-hung windows. Bay window on west side. Wood shingle siding; asphalt shingle roof. Terraced yard; set of five concrete steps with metal handrail. Asphalt driveway.

**22 Chestnut Street c. 1902**

**One and one-half story frame house with steeply pitched, cross-gambrel roof.**

Flat-roofed porch supported by broad round columns with decorative brick rail has overhanging bracketed eaves and flat roof; extension of porch to the east creates porte-cochere supported by fluted columns. Extension of porch does not appear original, due to differently spaced brackets and different column style, but does appear on 1930 Sanborn map. Porch shelters off-center front door, to the right (west) of which are two 1/1 double-hung windows. Palladianstyle window at second-floor front with solid sunburst above center window. Bay window on west side. Attached flat-roofed garage at southwest corner appears on 1930 Sanborn map; garage is accessed by a brick driveway. Wood shingle siding; asphalt shingle roof. Terraced yard; set of four concrete steps with modern wood rail.

 This house was occupied for about 60 years by two generations of the Moynihan family, passing from John P. and Alice Moynihan to their son, P. Seward Moynihan and his wife Dorothy.

**24 Chestnut Street c. 1920-30**

**Two-story frame house with steeply pitched, side-gambrel roof. Full-width front porch with slender square columns grouped in pairs and groups of three; porch has no rail and hipped roof**.

 Center entrance with group of three 6/1 double-hung wood windows to the left (east); paired 6/1 double-hung wood windows to the right (west). Second-floor front, projecting from gambrel, as paired casement at center and 8/1 double-hung wood sash to either side. One-story sun porch on east side. Terraced yard; concrete retaining wall with brick coping. Set of three concrete steps at center with wood rail; narrower set of four steps at west property line.

 Contributing one-story frame garage with flat roof and period door located just behind the house. Asphalt driveway.

**26 Chestnut Street c. 1901-1911**

**Two-story frame house with modest Queen Anne/Free Classic character; very similar to the house at 12 Chestnut Street.**

Hipped roof with front and side cross-gables. Full-width front porch has round columns, wood balustrade, and dentils at cornice. Porch shelters projecting entry vestibule with one window to either side. Second-floor front windows are 1/1 double-hung replacement sash. Bay window on west side. One-story shedroofed one-car garage attached on west side is not original. Vinyl siding; asphalt shingle roof. Terraced yard; set of four concrete steps with pipe handrail. Asphalt driveway.

**28 Chestnut Street c. 1915-20**

**Two-story frame house with American Foursquare form and Craftsman character.**

Side-gabled roof with deep overhang. Full-width front porch has tapered square posts on stone piers; wood balustrade; arched spandrels. Porch shelters center projecting vestibule with front door and sidelights. Chicago-style windows to either side of front vestibule consist of center 12/1 flanked by narrow 6/1 double-hung wood sash. Second-floor front windows are paired 12/1 double-hung wood sash. Shed-roofed front dormer contains bank of four 6/1 doublehung wood sash. Side window sizes and types vary, and include bank of three 6/1 double-hung wood sash in each gable. Rock-faced concrete block foundation; wood clapboard siding at first floor with wood shingle siding above. Asphalt shingle roof. Terraced yard; set of three concrete steps. This is a very good example of the American Foursquare form with Craftsman character.

 Contributing one-story frame garage with two garage bays and side-gabled roof; garage is a single structure that is shared between 28 and 30 Chestnut Street, half of which is on each property. Asphalt driveway.

**30 Chestnut Street c. 1901-11**

**Two-story frame house; front-gabled roof with cross-gable on west side.**

Full-width front porch has tapered square posts on rock-faced concrete block piers; solid sided balustrade. Porch shelters off-center front door in projecting enclosed vestibule, to the left (east) of which is one 1/1 double-hung wood window. Second-floor front windows are 1/1 double-hung sash and appear to be replacement units. Diminutive paired 1/1 windows in front gable. Bay window on east and west sides. Wood clapboard siding; wood shingles in gables. Terraced yard; set of three concrete steps.

 Half of the garage described under 28 Chestnut Street is on this property.

**32 Chestnut Street c. 1901-11**

**Two-story frame garage; front-gabled roof with cross-gable on west side.**

One-bay recessed porch at northwest corner, supported by square posts. To the left (east) of the porch is a bank of three 1/1 double-hung wood windows. Two second-floor front 1/1 double-hung windows. Pair of fixed/casement windows in front gable. Wood clapboard siding; wood shingle siding in gables; metal roof. Terraced yard; set of three concrete steps.

 Contributing one-story frame garage with shed roof. Concrete driveway shared with No. 34.

**34 Chestnut Street c. 1901-11**

**Two-story frame house with front-gabled roof and cross gable on west side.**

Entrance on west side sheltered by small pent-roofed entry porch. Center bay window at front has fixed front window, 12/12 windows to either side. Two second-floor front 1/1 double-hung replacement windows in reduced openings. Paired nine-lite fixed windows in front gable. Vinyl siding; asphalt shingle roof. This house has lost a front porch; vinyl siding, oversized bay window, and alterations to entry and fenestration reduce its integrity, but it retains its historic massing, which is similar to the houses at 32 and 30 Chestnut Street.

 Contributing one-story frame garage with gable roof.

**36 Chestnut Street c. 1901-11 Andrew J. Lawson, builder**

**Two-story frame house with front-gabled roof.**

 Full-with front porch has square columns and solid sided rail. Porch shelters off-center front door to left (east) and two 1/1 double-hung windows to the right (west). Fixed nine-lite window in gable. Aluminum siding; asphalt shingle roof. Terraced yard; set of three concrete steps.

 Contributing one-story frame garage with front-gabled roof. Concrete driveway.

**40 Chestnut Street 1907 Andrew J. Lawson, builder**

**Two-story frame house with front-gabled roof.**

Full-width front porch with hipped roof supported by square columns; no rail. Porch shelters projecting entry vestibule. One 1/1 double-hung window to the left (east) of vestibule; corner window to the right (west). Two second-floor front 1/1 double-hung replacement sash. Triple window in gable has tall center 1/1 double-hung sash flanked by shorter six-lite fixed or casement sash. West side has first-floor bay window and centered gable-roofed cross-gable dormer. Vinyl siding; asphalt shingle roof. Terraced yard; set of three concrete steps. Modern handrail.

 Contributing one-story frame gable-roofed garage. Asphalt driveway.

**42 Chestnut Street c. 1901-11**

**Two-story frame house with front-gabled roof.**

Full-width front porch, most of which is enclosed with vinylclad walls; modern bay window at front. Entrance is via small entry porch with entrance on west side of porch enclosure. Two second-floor front 1/1 double-hung replacement windows in reduced openings. Triple window in gable, with center window slightly taller than flanking windows. Bay window on west side. This house may originally have been similar to the neighboring house at 40 Chestnut Street, as the two have matching setbacks and similar rooflines; alterations to both have obscured possible other similarities. Extensive alterations to this house, including incompatible porch enclosure and modern window, alterations to fenestration, and vinyl siding, reduce integrity; it remains minimally contributing because it retains its historic massing.

 Contributing one-story frame garage with front-gabled roof. Concrete ribbon driveway infilled with asphalt.

**46 Chestnut Street c. 1920-30**

**Two-story frame house with Dutch Colonial Revival character; steeply pitched side-gambrel roof.**

Corner entry porch has slightly projecting hipped roof supported by decorative metal posts; entrance is recessed. Bank of three front 8/1 double-hung windows with period decorative shutters. Three second-floor front 8/1 wood windows, each with period decorative shutters, in pent-roofed projection. Wood shingle siding; asphalt shingle roof.

 Contributing one-story frame garage with closed-gable roof. Concrete driveway.

**50 Chestnut Street c. 1930**

**One-story frame bungalow with broad cross-**gable roof.

Partial-width projecting hip-roofed porch with period enclosure and solid sided rail. Left (east) of porch is a pair of 6/1 double-hung cottage-style windows. Triple window in front gable has taller central double-hung window flanked by half-height six-lite fixed windows, in upside-down Palladian configuration (windows align at lintels, rather than sills). Rock-faced concrete block foundation; wood clapboard siding at first story with wood shingle siding above.

 Contributing one-story frame garage with gable roof. Asphalt driveway.

**54 Chestnut Street c. 1915-25**

**Two-story frame house with American Foursquare form and Craftsman character.**

Full-width hip-roofed front porch with solid sided rail and square tapered posts; left (east) half of porch is enclosed with bank of 4/4 windows. Second-floor front 8/1 double-hung wood windows with period decorative shutters. Front and side hip-roofed dormers contain paired single-lite windows. Rock-faced concrete block foundation; wide clapboard siding; asphalt shingle roof.

 Contributing one-story frame garage with hipped roof. Concrete driveway.

**58 Chestnut Street c. 1920-30**

**Two-story frame house with side-gabled roof.**

Off-center front entrance sheltered by pedimented hood with square columns; door has narrow surround and diminutive fanlight. Left (east) of entrance is a bank of three 6/1 double-hung windows. Three evenly spaced second-floor front 6/1 double-hung wood windows. Pent-roofed sun porch on east side. Wood clapboard siding with cornerboards; asphalt shingle roof.

 Contributing one-story frame garage with side-gabled roof. Concrete driveway.

**62 Chestnut Street c. 1940**

 **One-story frame house with cross-gable roof.**

 Front-gabled wing has off-center front entrance with concrete stoop, to the left (east) of which are two 6/1 double-hung replacement windows. Vent in front gable. Picture window at front of west cross-gable wing. Attached one-story garage extends to west. Concrete driveway.

**68 Chestnut Street 1958 Romeo Biscaro, Builder**

**One-story house with rectangular footprint and low-pitched hipped roof.**

Small projecting hip-roofed entry porch, apparently unused and concealed by shrubs. Right (west) of porch is tripart picture window with brick sill; left (east) of porch are two smaller three-part windows with brick sills. House has stone veneer front and brick sides.

 Contributing one-story garage, also with stone veneer front and brick sides, with hipped roof. Asphalt driveway.

**76 Chestnut Street 1958 Romeo Biscaro, Builder**

**One-story house with hipped roof.**

 L-shaped footprint formed by main block of house to left (east) and attached garage to right (west). Primary entrance is on the west side of main house block and has low stoop, sheltered by deep overhang of hipped roof. Primary façade has large and small picture windows with brick sills. House and garage have stone veneer front and brick sides. Asphalt driveway.

**82 Chestnut Street 1958 Romeo Biscaro, Builder**

**Minimal Traditional/Ranch One-story house with rectangular footprint and low-pitched hipped roof.** Projecting hip-roofed overhang with slender metal posts on low stone wall shelters front entrance. Left (east) of front door is a wide three-part picture windows; shorter triple windows to right (west) of front door. Front and east sides have brick veneer below window sills and forming quoins around windows, door, and corner; brick infill between quoins. South and west sides are faced in brick.

 Contributing one-story hip-roofed garage to the south of house, with stone veneer front and brick sides. Concrete driveway.

**CHESTNUT STREET – NORTH SIDE (ODD)**

**9 Chestnut Street c. 1915-20**

**Two-story frame house with side-gabled roof; Colonial Revival and Craftsman character.**

Half-width recessed front porch has pent-roofed overhang, solid sided rail, and brick steps. To the right (east) of porch is a triple window, 12/1 double-hung wood sash at center flanked by narrow 6/1 double-hung wood sash. Center secondfloor front window is square with diamond muntin pattern; one 6/1 double-hung window to either side. Center front eyebrow dormer. Two-story projecting bay on east side. Wood shingle siding; asphalt shingle roof. Terraced yard; brick retaining wall and set of four brick steps to brick front wall. Asphalt driveway shared with No. 15.

**15 Chestnut Street c. 1915-20**

**Two-story frame house with American Foursquare form; hipped roof with side cross gables.**

 Full-width front porch has square columns, wood rail with square balusters, and flat roof. Porch shelters center front door with leaded-glass sidelights in enclosed projecting vestibule; one 1/1 double-hung wood window to either side. Two second-floor front 1/1 double-hung wood windows. Gable-roofed dormer with flat-topped Palladian window. Clapboard siding at first story, with wood shingle siding above. Terraced yard; brick retaining wall and set of four brick steps to brick front wall.

**17 Chestnut Street c. 1911-15**

**Two-story frame house with Craftsman character; low-pitched hipped roof with front and side gables.** Fullwidth front porch with tapered square columns; square balusters. Porch shelters center front door with leadedglass sidelights in enclosed projecting vestibule; cottage-style 1/1 double-hung wood window to either side. Two pairs of second-floor front 1/1 double-hung wood windows. Deeply overhanging, bracketed eaves. Three square 2/2 windows in each dormer. Vinyl siding; asphalt shingle roof. Terraced yard; brick retaining wall with concrete coping. Four brick and concrete steps.

 Contributing one-story frame garage with hipped roof. Asphalt driveway shared with No. 19.

**19 Chestnut Street c. 1911-15**

**Two-story frame house with front-gabled roof.**

Full-width, hip-roofed front porch with solid shingle-sided rail and corner posts, and arched openings. Porch shelters center front door with 1/1 double-hung replacement sash to either side. Porch is entered from west side. Two 1/1 double-hung front second-floor windows. Paired windows in gable. Enclosed entry vestibule on west side with hipped roof. Wood ribbon-coursed shingle siding; asphalt shingle roof. Terraced yard; brick retaining wall with concrete coping. St of four concrete steps with modern handrail.

 Contributing one-story frame garage with front-gabled roof and ribbon-coursed shingle siding.

**21 Chestnut Street c. 1901-1911**

 **Two-story frame house with Colonial Revival form and Craftsman features.**

Side-gabled roof. Full-width, pent-roofed front porch with period enclosure created by banks of windows. Center front door flanked by pilasters. Three second-floor front 1/1 double hung windows; center window is smaller than the other two. Gable-roofed front dormer. Porch roof and main roof have bracketed eaves and exposed rater tails. Bay window on east and sides. Terraced yard; set of four concrete steps with pipe handrail.

 Contributing one-story frame garage with projecting gable. Concrete driveway shared with No. 23.

**23 Chestnut Street c. 1911-15**

**Two-story frame house with front-gabled roof.**

Full-width front porch has metal rail and posts (not original) supporting hipped roof. Porch shelters center front door with one 1/1 double-hung replacement window to either side. Two second-floor front 1/1 double-hung replacement windows. Bay window on west side. Aluminum and vinyl siding; asphalt shingle roof. Terraced yard; set of five concrete steps.

 One-story frame garage with front-gabled roof.

**25 Chestnut Street c. 1920-30**

**Two-story frame house with front-gabled roof.**

Full-width front porch has round columns, no rail, and hipped roof. Porch shelters front door to right (east) and bay window containing five 1/1 double-hung replacement sash to left (west). Second-floor front has two pairs of 6/1 windows flanking smaller center six-lite window. Paired 6/1 wood windows in gable. Bay window on west side. Rock-faced concrete block foundation; vinyl siding; asphalt shingle roof. Terraced yard; set of five concrete steps that appear modern. Modern rail.

 Contributing one-story frame garage with front-gabled roof. Concrete driveway.

**27 Chestnut Street c. 1911-15**

**Two-story frame house with American Foursquare form and modest Colonial Revival character.**

Full-width front porch with square wood posts, in groups of three at corners and paired at center, and wood balustrade. Porch shelters off-center front door with 1/1 cottage-style window to left (west) and 1/1 window to right (east). Two second-floor front 1/1 windows with smaller fixed window between them. Hip-roofed front and side dormers. Clapboard siding at first floor, except on west side where there is vertical board siding. Second-floor siding is wood shingles. Asphalt shingle roof. Terraced yard; set of four brick steps. Contributing one-story frame garage with gable roof. Asphalt driveway.

**31 Chestnut Street c. 1915-20**

**Two-story frame house with side-gabled roof.**

Projecting entry vestibule contains front door with sidelights and has a low-pitched hipped roof. Triple windows to either side consist of one 6/6 double-hung sash flanked by narrow 1/1 sash. Second-floor front windows are paired 6/6 double-hung sash. Side window sizes and configurations vary and include triple windows in each gable end. Windows generally appear to be replacement units. Clapboard siding at first floor with wood shingles above. 1930 Sanborn map shows full-width front porch, now missing. Terraced yard; lumber retaining wall with set of six lumber and brick steps.

 Contributing one-story frame garage with side-gabled roof. Concrete and brick driveway.

**33 Chestnut Street c. 1915-20**

**Two-story frame house with side-gambrel roof.**

Center entry sheltered by projecting gable-roofed portico supported by paired fluted columns; door has sidelights and blind decorative fanlight. Triple windows to either side of entrance are wood 6/1 flanked by 4/1 double-hung sash to right (east) of entrance; triple window to left (west) of entrance contains three 1/1 double-hung replacement sash. Second-floor front windows, in shed roofed dormer, are paired 1/1 replacement sash to either side of a pair of smaller six-lite wood windows. Flatroofed sun porch projects on east side. Clapboard siding; asphalt shingle roof. Terraced yard; brick retaining wall with set of four brick and concrete steps.

 Contributing one-story frame garage has gambrel roof with shed dormer. Asphalt driveway.

**37 Chestnut Street c. 1922**

**One-story bungalow with stucco exterior; side-gabled roof.**

Nearly full-width front porch has squat square posts on battered stucco-clad piers, between which is a distinctive rail solid at the bottom with short balusters above. Entablature incorporates a decorative band resembling another row of balusters. Porch roof has front-facing gable roof supported by brackets, and has exposed rater tails. Main roof also has brackets and exposed rafter tails. Porch shelters center front door with paired 6/1 cottage-style windows to either side. Bay window on east and west sides. Stucco exterior; asphalt shingle roof. This is a distinctive and highly intact example of the Craftsman style and is one of the most architecturally notable houses on Chestnut Street. Terraced yard; set of five concrete steps.

 Contributing one-story frame gable-roofed garage. Concrete driveway.

**41 Chestnut Street c. 1920-30**

**Two-story frame house with side-gabled roof.**

Front central cross-gable is slightly projected above first floor. Off-center front door to left (west) of cross-gable has pedimented hood on turned posts (these do not appear original). To the right (east) of front door, beneath projecting cross-gable, is a bank of three fixed or casement windows with no muntins. Pair of 1/1 windows at right. Second-floor front windows are bank of three 1/1 replacement sash in cross gable; one 1/1 window in shed-roofed wall dormer to either side. Vinyl siding, with artificial shingle in front cross-gable; asphalt shingle roof. This is an unusual form but is generally comparable to what appears on the 1930 map; one difference is that the 1930 map shows an open, possibly recessed, porch at right front (southeast) corner. Terraced yard; set of three concrete steps.

 Contributing one-story frame garage with side-gabled roof. Concrete driveway.

**43 Chestnut Street c. 1922**

**One and one-half story frame house with side gabled roof.**

Slightly projecting front cross-gable contains front door, which is topped by an elongated swans-neck hood. Short 6/6 double-hung window with half-round fanlight above front door. Pair of windows to left (west) of front door; triple window to the right. Two front dormers: left-hand (west) dormer has a gable roof and contains a one-lite window; right-hand (east) dormer is a wall dormer with gable roof. Windows appear to be a mix of wood sash and replacement units. Aluminum siding; asphalt shingle roof. Although its form suggests a later construction date, this house is mentioned in newspaper articles dating back to 1922, when it was described as Mr. and Mrs. Marvin Wilson’s “new home.” Terraced yard; set of three brick steps integral with brick front walk.

 Contributing one-story frame garage with gambrel roof. Concrete driveway (new) shared with No. 47.

**47 Chestnut Street c. 1923**

 **Two-story frame house with side-gambrel roof.**

Center entrance has gabled hood supported by slender paired columns. Front door has sidelights; door and sidelights framed by slender pilasters. One 8/1 double-hung wood window with period decorative shutters to either side of door. Pent roof across front wraps both sides. Three 1/1 double-hung second-floor windows in broad shed dormer. Clapboard siding; asphalt shingle roof. Terraced yard; set of three brick steps integral with brick front walk.

 Contributing one-story frame garage with gambrel roof.

**51 Chestnut Street c. 1930**

**Frame bungalow, one and one-half stories plus attic.**

Full-width front porch beneath main roof is supported by squat battered posts on solid sided rail. Porch shelters off-center front door at right (east), with bank of three 1/1 double-hung windows to left. Broad shed dormer contains two pairs of short 1/1 double-hung windows. Windows generally appear to be replacement units. Main roof and shed dormer roof have brackets at eaves and exposed rafter tails. Bay window on west side. Clapboard siding at first floor with wood shingle siding above; asphalt shingle roof. Terraced yard; set of three concrete steps.

 Contributing one-story frame gable-roofed garage. Concrete driveway.

**55 Chestnut Street c. 1930**

**Two-story frame house with side-gabled roof.**

Symmetrical façade; center entrance consists of front door with sidelights accessed by brick steps and stoop, sheltered by gable-roofed entry porch supported by square columns. Paired 6/6 double-hung replacement windows to either side of front entrance. Three second-floor front 6/6 double-hung replacement windows; center window shorter than the other two. Symmetrical east and west sides, each with short paired 1/1 windows at first floor and standard sized 6/6 replacement sash at second floor; west side also has brick chimney. Siding appears to be aluminum. Asphalt shingle roof. Terraced yard; set of three concrete steps.

Contributing one-story frame garage with side-gabled roof. Concrete driveway.

**59 Chestnut Street c. 1910-20**

**One and one-half story frame bungalow with steeply pitched side-gabled roof.**

Full-width front porch beneath main roof, supported by tapered square columns on cast-concrete posts with solid sided rail. Porch shelters center front door in projecting vestibule. Chicago-style triple window to either side of front door, with Craftsman-style sash featuring four vertical lites in upper center sash. Shed-roofed front dormer contains bank of three windows of similar Craftsman style with three vertical lites in upper sash; shed dormer roof has exposed rafter tails. Bay window on east side. This is a very good example of a Craftsman-style bungalow with high integrity. Terraced yard; set of three concrete steps.

 Contributing one-story frame garage with front-gabled roof. Concrete driveway.

**63 Chestnut Street c. 1915-20**

**One and one-half story frame bungalow with steeply pitched side-gabled roof.**

Full-width front porch beneath main roof, supported by tapered square columns on rock-faced concrete-block piers with wood balustrade. Porch shelters off-center front door; first-floor fenestration concealed by coniferous bushes in front of porch. Broad front shed dormer contains four 6/1 double-hung wood windows with fixed six-lite window at center. Bay window on west side. Vinyl siding; asphalt shingle roof. Terraced yard; set of three concrete steps (new) with metal rail.

 Contributing one-story frame garage with front-gabled roof. Asphalt driveway.

**67 Chestnut Street c. 1915-20**

**One and one-half story frame bungalow with steeply pitched side-gabled roof.**

Full-width front porch, beneath main roof, has unusual configuration: wide tapered square wood columns are set on cast concrete-block piers, inset from corners. Balustrade extends past piers to porch corners and has square balusters and posts. Porch shelters off-center front door to right (east) with bank of three 1/1 double-hung replacement windows to left (west). Front gable-roofed dormer contains bank of three 1/1 double-hung replacement windows. Bay window on west side. Aluminum siding; asphalt shingle roof. Terraced yard; set of three concrete steps.

 Contributing one-story frame garage with front-gabled roof. Concrete driveway.

**81 Chestnut Street c. 1950**

**Two-story frame house with mid-20th century Colonial Revival character.**

 Front entrance is located in a projecting shed-roofed vestibule whose roof and front wall are continuous with the attached garage to the west. Modern stoop/deck in front of porch has tall vinyl balustrade. To the right of the entry vestibule is a picture window flanked by 8-lite casements. Two second-floor front 8/8 double-hung windows. Brick chimney on east side. Vinyl siding; asphalt shingle roof. Asphalt driveway.