**WINSOR STREET – WEST SIDE (ODD)**

 **625 Winsor Street c. 1928**

**Two-story house with side-gabled roof and formal Colonial Revival character.**

Center entrance sheltered by portico featuring fluted Corinthian columns, dentilled cornice, and roof balustrade. Front door is flanked by sidelights and has semi-elliptical transom. Single 6/6 window to either side of entrance, aligned with similar 6/6 windows at second-floor front. Second-floor center door above entry. Modillions at eaves. Two-story pilasters inset from corners. Attached garage at northwest corner, accessed by an asphalt driveway. Wide clapboard siding; asphalt shingle roof. Metal fence at perimeter appears modern.

**629 Winsor Street c. 1911**

**Designed by Freeburg & Fidler Two-story Craftsman-style house with broad gable-on-hip roof and battered sides.**

Center entrance in projecting gable-roofed vestibule. First-floor windows are paired 8/8 double-hung replacement sash; secondfloor windows are 6/6 double-hung sash. Dormer on south side with thatch-style curved roof. Front eaves have eyebrow arch at center. Wood shingle siding; asphalt shingle roof. In the front yard are three large mature trees; the sidewalk in front of this house bows out into the space normally occupied by the grassy apron, to accommodate these trees. Two concrete retaining walls with brick coping are situated between the trees and sidewalk.

 Contributing frame one-story garage with hipped roof.

**633 Winsor Street c. 1900**

**Two- story, front-gabled house with simple, vernacular form.**

Full-width front porch with paired square columns, deck-style balustrade, and flat roof. Porch shelters off-center front door and two 1/1 double-hung windows, which are aligned with second-floor front windows. Bay window on right (north) side.

 Contributing one-story frame garage; asphalt driveway.

**WINSOR STREET – EAST SIDE**

**628 Winsor Street c. 1913**

**One-and-one-half-story bungalow on large corner lot, placed at an angle to the street.**

Broad side-gambrel roof with large shed dormer. Roof extends to shelter a full-width front porch with square columns. Projecting entry vestibule; front door has sidelights. Window are generally 1/1 double-hung replacement sash. Vinyl siding; prominent blue metal roof. Terraced yard; set of two new concrete steps with metal handrails. Attached garage on east side; asphalt driveway.

**630 Winsor Street c. 1913**

**Two-story frame house with side-gabled roof.**

Full-width front porch with battered square posts and wood balustrade. Central front door with sidelights; 12/1 window with sidelights to either side. Second-floor front windows are paired 9/1 double-hung sash. Wide shed dormer with three six-pane wood windows. Wood shingle siding; asphalt shingle roof. Terraced yard; set of three concrete steps.

 Contributing one-story frame garage with hipped roof. Concrete driveway shared with 632 Winsor Street.

**632 Winsor Street c. 1916**

**One-story bungalow with side-gabled roof.**

Broad, low-pitched, side-gabled roof with gabled and shed dormers and broad overhanging eaves; roof shelters a full-width front porch with brick posts. Brick exterior at first floor with wood shingles in gable ends and at dormer. Variety of window shapes and types. Terraced yard; set of four concrete steps. House retains a high degree of integrity of design, materials, and craftsmanship.

**636 Winsor Street c. 1917**

**This sophisticated and picturesque Tudor Revival-style residence has a steeply pitched, cross-gable roof with half-timbering in the front gable end.**

Projecting gabled entry porch with square stucco posts, brackets, and irregular clapboard siding in gable end; shape of this porch is echoed in adjacent porte-cochere. Stonework at porch and porte-cochere flows into low stone retaining walls lining driveway and sidewalk, which have two integral sets of stone steps at public sidewalk. Banks of leaded-glass double-hung and casement windows. Rough stucco exterior with stone detailing; asphalt shingle roof. Attached garage at rear.

**642 Winsor Street c. 1912**

**Two and one-half story frame house with hipped roof and hipped dormers.**

Full-width, one-story front porch with grouped Ionic columns on rusticated concrete-block pedestals. Smaller half-width front second-floor porch. Hip-roofed front and side dormers contain triple 6/1 double-hung wood sash. Bay window on left (north) side; open side porch on right (south) side. Rusticated concrete block foundation; wood clapboard and shingle siding; asphalt shingle roof. Terraced lot; set of three concrete steps with metal handrails.

 Contributing one-story frame garage; concrete driveway.

**650 Winsor Street c. 1905 Carl C. Pedersen, Architect**

**Two-and-one-half-story, front gambrel, frame house situated at an angle on a corner lot.**

Full-width front porch with square posts on solid aluminum sided rail. Porch shelters off-center front door with picture window to the left and double-hung window with sidelights to right. Second-floor front oriel window. Aluminum siding; asphalt shingle roof. Simple metal fence.

 One-story frame garage with hipped roof; asphalt driveway.

 This house was one of several in the district that were pictured in an article about architect Carl C. Pedersen in The Ohio Architect, Engineer and Builder (July 1913).